Downloading Wind Data

1. Use the 2 keys to open the data collection box at wind sensor.
2. Connect cable to data logger and USB to the upper right USB inlet on the field laptop.
3. Start laptop and login.
4. Open the program “PC200W” (close utility window of the program if that pops up as well).
5. Click “Connect” at top left corner of window (computer should look for wind logger and connect).
6. Click “Collect data” tab.
7. Chose “collect new data only” and start collecting.
8. It’ll take a few minutes to download approx. 80,000 readings.
9. Once finished downloading, you get the option to view the data or just close the window.
10. The program automatically saves the data under a generic name in C\Campbellsci\PC200W. Go into the folder and change the name of the file, otherwise the program will overwrite this file next time!!
11. Click “Disconnect” on the PC200W program and disconnect data logger.
12. Close and lock up wind sensor box.